These musebots were made in Whistler June 9-14 to work with the new Downbeat / SubConductor model.

They receive messages on their individual ports (displayed in their main window).

They send messages on port 6000.

You will need to set the IP number on the bot. The last number isn’t needed, as it is set to 255, which means it will transmit to all computers on the network.

Don’t select “Ethernet”, unless you set ALL computers to be on IP 1.1.1.x, with x being a unique number for each computer.